*HEADING
**
** Creep analysis of a rod.
** Verification of *HYPERELASTIC, MARLOW and *VISCOELASTIC
** incompressible
**
*PREPRINT, MODEL=YES
*NODE,NSET=ALL
*nset,nset=nx0
*nset,nset=nx1
*nset,nset=ny0
*nset,nset=nz0
*NSET, NSET=NDISP
*ELEMENT,TYPE=T3D2,ELSET=ONE
*ELEMENT,TYPE=c3d8rh,ELSET=two
*elset,elset=eall
*SOLID SECTION,ELSET=eall,MATERIAL=MAT1
*MATERIAL,NAME=MAT1
*HYPERELASTIC,MARLOW, MODULI = INSTANTANEOUS
*UNIAXIAL TEST DATA
*VISCOELASTIC,TIME=RELAXATION TEST DATA
*COMBINED TEST DATA,SHRINF=0.50,VOLINF=0.50
*STEP, NLGEOM
 UNIAXIAL LOADING
*STATIC
 0.01,1.0,,0.05
*BOUNDARY
 1,1,3
 2,2,3
nx0,1,1
ny0,2,2
nz0,3,3
*CLOAD
 2,1,65.0E5
nx1,1,16.25E5
*OUTPUT,FIELD, VARIABLE=PRESELECT
*OUTPUT, HISTORY, VARIABLE=PRESELECT
*ELEMENT OUTPUT, ELSET=eall
 S11, LE11, NE11, EE11, CE11, cener
*NODE OUTPUT, NSET=NDISP
U1
*END STEP
*STEP, NLGEOM
 SUSTAIN LOAD
*VISCO
 5.,100.,2.,10.,
*END STEP