*HEADING
 Transfer from Standard to Explicit:  Test for B31 element
 - Explicit analysis
 - further loading of the tension
*IMPORT,UPDATE=YES,STATE=YES
 RECT, BOX, CIRC, HEX, I, L, PIPE, TRAP
*IMPORT NSET
 ALL, LEFT, RIGHT , QA_TEST_ALLNODES
*IMPORT ELSET
 QA_TEST_ALLELEMS
*BOUNDARY
 LEFT, 1,6
 RIGHT, 2,6
**
*AMPLITUDE,NAME=AMP1,DEFINITION=SMOOTH
0,0,0.1,1.0
*STEP
*DYNAMIC,EXPLICIT
 , 0.1
*BOUNDARY,TYPE=VELOCITY,AMPLITUDE=AMP1
RIGHT,1,1,0.5
*OUTPUT,FIELD,VARIABLE=PRESELECT
**FOR QA PURPOSE
*OUTPUT, FIELD, TIMEMARKS=YES, NUMBER INTERVAL=4
*ELEMENT OUTPUT,ELSET=QA_TEST_ALLELEMS
 LE,
*NODE OUTPUT,NSET=QA_TEST_ALLNODES
COORD,UT
*OUTPUT,HISTORY,TIME INTERVAL=0.01
*ENERGY OUTPUT
ALLIE,ALLKE,ALLSE,ALLWK,ETOTAL
*END STEP