*HEADING
  TEST SUBSTRUCTURE BETA DAMPING FOR DIRECT INTEGRATION
** TEST OVERRIDE OF DAMPING PROPERTIES ON THE *SUBSTRUCTURE PROPERTY OPTION
*NODE, NSET=NALL
*ELEMENT,TYPE=Z01,ELSET=TRUSS,FILE=rayleighdamping_substr_alpha_gen1
*SUBSTRUCTURE PROPERTY,ELSET=TRUSS
*DAMPING,BETA=1.59248E-3
*STEP
*STATIC
*BOUNDARY
1,1,3
2,2,3
2,1,,1.
*PRINT,RESIDUAL=NO,FREQUENCY=5
*SUBSTRUCTURE PATH,ENTER ELEMENT=1
*OUTPUT,FIELD,VAR=PRESELECT
*EL FILE,FREQUENCY=25
S,E
*EL PRINT,FREQUENCY=25,SUMMARY=NO
S,E
*SUBSTRUCTURE PATH,LEAVE
*NODE FILE,FREQUENCY=5
U,
*NODE PRINT,FREQUENCY=5,SUMMARY=NO
U1,V1,A1,RF1
*OUTPUT, FIELD, FREQUENCY=999
*NODE OUTPUT, NSET=NALL
U,
*ELEMENT OUTPUT, ELSET=TRUSS
S,E
*OUTPUT, HISTORY, FREQUENCY=5
*NODE OUTPUT, NSET=NALL
U,
*ELEMENT OUTPUT, ELSET=TRUSS
S,E
*END STEP
*STEP,INC=300
*DYNAMIC,ALPHA=0.,DIRECT
.01,2.5
*BOUNDARY,OP=NEW
1,1,3
2,2,3
*END STEP