*HEADING
 Test import capability:     CPS4R
 UNIAXIAL STRETCHING OF A RUBBER SHEET  sx_x_holehyper.inp
 W/ CIRCULAR HOLE - PLANE STRESS
 Results imported from: sx_s_holehyper.inp
 Base for file:         xs_s_holehyper.inp
*IMPORT,STEP=1,UPDATE=NO,STATE=YES
 ALLE,
*RESTART,TIMEMARKS=YES,WRITE
*EQUATION
RMPC,1,1.,1601,1,-1.
*STEP
*DYNAMIC,EXPLICIT, IMPROVED DT METHOD=NO
  ,1.0
*BOUNDARY,TYPE=VELOCITY
BOTTOM,2
TOP,2
LEFT,1
1601,1,,7.0
*file output,num=1
*NODE FILE
 U,
*EL FILE
***OUTPUT,HISTORY,TIME INTERVAL=0.0
***NODE OUTPUT,nset=RMPC
**U,
*VARIABLE MASS SCALING, TYPE=BELOW MIN, DT=1.0E-03, FREQ=30
*OUTPUT,FIELD,NUMBER INTERVAL=1
*ELEMENT OUTPUT
S,
LE,
PE,
*NODE OUTPUT
COORD,
*END STEP