*HEADING
Implicit verification for meshed general section
*PREPRINT,ECHO=YES,MODEL=YES,HISTORY=YES
*PART, NAME=LINEARMESHED
*NODE
*NGEN,NSET=ALL
*ELEMENT,TYPE=B31, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=MESHED,ELSET=EALL
0., 0., -1.
*INCLUDE,INPUT=meshedsect_i_iso.bsp
*END PART
*PART, NAME=QUADRATICMESHED
*NODE
*NGEN,NSET=ALL
*ELEMENT,TYPE=B32, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=MESHED,ELSET=EALL
0., 0., -1.
*INCLUDE,INPUT=meshedsect_i_iso.bsp
*END PART
*PART, NAME=LINEARGENERAL
*NODE
*NGEN,NSET=ALL
*ELEMENT,TYPE=B31, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=GENERAL,DENSITY=7.3E-4,ELSET=EALL
2.26E+1,3.07358E+2,2.3711E-3,.54034333E+2,9.99
0., 0., -1.
3.E+7, 1.1538451E+7,
*centroid
*shear center
*END PART
*PART, NAME=QUADRATICGENERAL
*NODE
*NGEN,NSET=ALL
*ELEMENT,TYPE=B32, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=GENERAL,DENSITY=7.3E-4,ELSET=EALL
2.26E+1,3.07358E+2,2.3711E-3,.54034333E+2,9.99
0., 0., -1.
3.E+7, 1.1538451E+7,
*centroid
*shear center
*END PART
*ASSEMBLY, NAME=ASSEMBLY
*INSTANCE,NAME=LINEARMESHED_A, PART=LINEARMESHED
*END INSTANCE
*INSTANCE,NAME=QUADRATICMESHED_A, PART=QUADRATICMESHED
*END INSTANCE
*INSTANCE,NAME=LINEARGENERAL_A, PART=LINEARGENERAL
*END INSTANCE
*INSTANCE,NAME=QUADRATICGENERAL_A, PART=QUADRATICGENERAL
*END INSTANCE
*END ASSEMBLY
*BOUNDARY
ASSEMBLY.LINEARMESHED_A.1, 1, 6
ASSEMBLY.QUADRATICMESHED_A.1, 1, 6
ASSEMBLY.LINEARGENERAL_A.1, 1, 6
ASSEMBLY.QUADRATICGENERAL_A.1, 1, 6
*NSET, NSET=QA_TEST_NALL
ASSEMBLY.LINEARMESHED_A.11
ASSEMBLY.QUADRATICMESHED_A.11
ASSEMBLY.LINEARGENERAL_A.11
ASSEMBLY.QUADRATICGENERAL_A.11
*ELSET, ELSET=QA_TEST_EALL
ASSEMBLY.LINEARMESHED_A.1
ASSEMBLY.QUADRATICMESHED_A.1
ASSEMBLY.LINEARGENERAL_A.1
ASSEMBLY.QUADRATICGENERAL_A.1
*STEP,inc=1000
*DYNAMIC,direct
0.0001,0.1
*CLOAD
ASSEMBLY.LINEARMESHED_A.11,2,2.5E+5
ASSEMBLY.QUADRATICMESHED_A.11,2,2.5E+5
ASSEMBLY.LINEARGENERAL_A.11,2,2.5E+5
ASSEMBLY.QUADRATICGENERAL_A.11,2,2.5E+5
*EL PRINT,ELSET=QA_TEST_EALL,FREQ=1000
S,
E,
*EL FILE,ELSET=QA_TEST_EALL,FREQ=1000
E,
*OUTPUT,FIELD,FREQ=1000
*NODE OUTPUT, NSET=QA_TEST_NALL
U,
*ELEMENT OUTPUT,ELSET=QA_TEST_EALL
SE,
S,
*OUTPUT, HISTORY,FREQ=10
*NODE OUTPUT, NSET=QA_TEST_NALL
U,
*ELEMENT OUTPUT,ELSET=QA_TEST_EALL
S,
*END STEP